# RBR_DLL_THR in k210_pac::uart1 - Rust
Receive Buffer Register / Divisor Latch (Low) / Transmit Holding Register (depending on context and R/W)
Keywords: rust, rustlang, rust-lang, RBR_DLL_THR

# Type Definition k210_pac::uart1::RBR_DLL_THR

source · [−]

    pub type RBR_DLL_THR = Reg<u32, _RBR_DLL_THR>;

Expand description

Receive Buffer Register / Divisor Latch (Low) / Transmit Holding Register (depending on context and R/W)

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rbr_dll_thr module

## Trait Implementations

source

### impl ResetValue for RBR_DLL_THR

Register rbr_dll_thr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RBR_DLL_THR

`read()` method returns rbr_dll_thr::R reader structure

source

### impl Writable for RBR_DLL_THR

`write(|w| ..)` method takes rbr_dll_thr::W writer structure