# CTL in k210_pac::dmac::channel - Rust
Control Register
Keywords: rust, rustlang, rust-lang, CTL

# Type Definition k210_pac::dmac::channel::CTL

source · [−]

    pub type CTL = Reg<u64, _CTL>;

Expand description

Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ctl module

## Trait Implementations

source

### impl ResetValue for CTL

Register ctl `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CTL

`read()` method returns ctl::R reader structure

source

### impl Writable for CTL

`write(|w| ..)` method takes ctl::W writer structure