# RXFLR in k210_pac::spi3 - Rust
Receive FIFO Level Register
Keywords: rust, rustlang, rust-lang, RXFLR

# Type Definition k210_pac::spi3::RXFLR

source · [−]

    pub type RXFLR = Reg<u32, _RXFLR>;

Expand description

Receive FIFO Level Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxflr module

## Trait Implementations

source

### impl ResetValue for RXFLR

Register rxflr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXFLR

`read()` method returns rxflr::R reader structure

source

### impl Writable for RXFLR

`write(|w| ..)` method takes rxflr::W writer structure