# INTERRUPT_MASK in k210_pac::kpu - Rust
Interrupt mask: 0 enables the interrupt, 1 masks the interrupt
Keywords: rust, rustlang, rust-lang, INTERRUPT_MASK

# Type Definition k210_pac::kpu::INTERRUPT_MASK

source · [−]

    pub type INTERRUPT_MASK = Reg<u64, _INTERRUPT_MASK>;

Expand description

Interrupt mask: 0 enables the interrupt, 1 masks the interrupt

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see interrupt_mask module

## Trait Implementations

source

### impl ResetValue for INTERRUPT_MASK

Register interrupt_mask `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for INTERRUPT_MASK

`read()` method returns interrupt_mask::R reader structure

source

### impl Writable for INTERRUPT_MASK

`write(|w| ..)` method takes interrupt_mask::W writer structure