# k210_pac::dmac::channel - Rust
Register block Channel configuration
Keywords: rust, rustlang, rust-lang, channel

# Module k210_pac::dmac::channel

source · [−]
Expand description

Register block Channel configuration

## Modules

_reserved

Padding to make structure size 256 bytes so that channels[] is an array

axi_id

Channel AXI ID Register

axi_qos

AXI QOS Register

blk_tfr

Channel Block Transfer Resume Request Register

block_ts

Block Transfer Size Register

cfg

Configure Register

ctl

Control Register

dar

DAR Address Register

intclear

Interrupt Clear Register

intsignal_en

Interrupt Signal Enable Register

intstatus

Channel Interrupt Status Register

intstatus_en

Interrupt Status Enable Register

llp

Linked List Pointer register

sar

SAR Address Register

status

Channel Status Register

swhsdst

Channel Software handshake Destination Register

swhssrc

Channel Software handshake Source Register

## Type Definitions

AXI_ID

Channel AXI ID Register

AXI_QOS

AXI QOS Register

BLK_TFR

Channel Block Transfer Resume Request Register

BLOCK_TS

Block Transfer Size Register

CFG

Configure Register

CTL

Control Register

DAR

DAR Address Register

INTCLEAR

Interrupt Clear Register

INTSIGNAL_EN

Interrupt Signal Enable Register

INTSTATUS

Channel Interrupt Status Register

INTSTATUS_EN

Interrupt Status Enable Register

LLP

Linked List Pointer register

SAR

SAR Address Register

STATUS

Channel Status Register

SWHSDST

Channel Software handshake Destination Register

SWHSSRC

Channel Software handshake Source Register

_RESERVED

Padding to make structure size 256 bytes so that channels[] is an array