# IV in k210_pac::aes - Rust
Initialisation Vector (96 bit for GCM, 128 bit for CBC)
Keywords: rust, rustlang, rust-lang, IV

# Type Definition k210_pac::aes::IV

source · [−]

    pub type IV = Reg<u32, _IV>;

Expand description

Initialisation Vector (96 bit for GCM, 128 bit for CBC)

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see iv module

## Trait Implementations

source

### impl ResetValue for IV

Register iv[%s] `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for IV

`read()` method returns iv::R reader structure

source

### impl Writable for IV

`write(|w| ..)` method takes iv::W writer structure