# k210_pac::sysctl::peri - Rust
Peripheral controller
Keywords: rust, rustlang, rust-lang, peri

# Module k210_pac::sysctl::peri

source · [−]
Expand description

Peripheral controller

## Structs

DEBUG_CLK_BYPASS_W

Write proxy for field `debug_clk_bypass`

DVP_CLK_BYPASS_W

Write proxy for field `dvp_clk_bypass`

I2S0_CLK_BYPASS_W

Write proxy for field `i2s0_clk_bypass`

I2S1_CLK_BYPASS_W

Write proxy for field `i2s1_clk_bypass`

I2S2_CLK_BYPASS_W

Write proxy for field `i2s2_clk_bypass`

JTAG_CLK_BYPASS_W

Write proxy for field `jtag_clk_bypass`

SPI0_CLK_BYPASS_W

Write proxy for field `spi0_clk_bypass`

SPI0_XIP_EN_W

Write proxy for field `spi0_xip_en`

SPI1_CLK_BYPASS_W

Write proxy for field `spi1_clk_bypass`

SPI1_XIP_EN_W

Write proxy for field `spi1_xip_en`

SPI2_CLK_BYPASS_W

Write proxy for field `spi2_clk_bypass`

SPI2_XIP_EN_W

Write proxy for field `spi2_xip_en`

SPI3_XIP_EN_W

Write proxy for field `spi3_xip_en`

TIMER0_PAUSE_W

Write proxy for field `timer0_pause`

TIMER1_PAUSE_W

Write proxy for field `timer1_pause`

TIMER2_PAUSE_W

Write proxy for field `timer2_pause`

TIMER3_PAUSE_W

Write proxy for field `timer3_pause`

TIMER4_PAUSE_W

Write proxy for field `timer4_pause`

TIMER5_PAUSE_W

Write proxy for field `timer5_pause`

TIMER6_PAUSE_W

Write proxy for field `timer6_pause`

TIMER7_PAUSE_W

Write proxy for field `timer7_pause`

TIMER8_PAUSE_W

Write proxy for field `timer8_pause`

TIMER9_PAUSE_W

Write proxy for field `timer9_pause`

TIMER10_PAUSE_W

Write proxy for field `timer10_pause`

TIMER11_PAUSE_W

Write proxy for field `timer11_pause`

## Type Definitions

DEBUG_CLK_BYPASS_R

Reader of field `debug_clk_bypass`

DVP_CLK_BYPASS_R

Reader of field `dvp_clk_bypass`

I2S0_CLK_BYPASS_R

Reader of field `i2s0_clk_bypass`

I2S1_CLK_BYPASS_R

Reader of field `i2s1_clk_bypass`

I2S2_CLK_BYPASS_R

Reader of field `i2s2_clk_bypass`

JTAG_CLK_BYPASS_R

Reader of field `jtag_clk_bypass`

R

Reader of register peri

SPI0_CLK_BYPASS_R

Reader of field `spi0_clk_bypass`

SPI0_XIP_EN_R

Reader of field `spi0_xip_en`

SPI1_CLK_BYPASS_R

Reader of field `spi1_clk_bypass`

SPI1_XIP_EN_R

Reader of field `spi1_xip_en`

SPI2_CLK_BYPASS_R

Reader of field `spi2_clk_bypass`

SPI2_XIP_EN_R

Reader of field `spi2_xip_en`

SPI3_XIP_EN_R

Reader of field `spi3_xip_en`

TIMER0_PAUSE_R

Reader of field `timer0_pause`

TIMER1_PAUSE_R

Reader of field `timer1_pause`

TIMER2_PAUSE_R

Reader of field `timer2_pause`

TIMER3_PAUSE_R

Reader of field `timer3_pause`

TIMER4_PAUSE_R

Reader of field `timer4_pause`

TIMER5_PAUSE_R

Reader of field `timer5_pause`

TIMER6_PAUSE_R

Reader of field `timer6_pause`

TIMER7_PAUSE_R

Reader of field `timer7_pause`

TIMER8_PAUSE_R

Reader of field `timer8_pause`

TIMER9_PAUSE_R

Reader of field `timer9_pause`

TIMER10_PAUSE_R

Reader of field `timer10_pause`

TIMER11_PAUSE_R

Reader of field `timer11_pause`

W

Writer for register peri