# RAR in k210_pac::uart1 - Rust
Receive-Mode Address Register
Keywords: rust, rustlang, rust-lang, RAR

# Type Definition k210_pac::uart1::RAR

source · [−]

    pub type RAR = Reg<u32, _RAR>;

Expand description

Receive-Mode Address Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rar module

## Trait Implementations

source

### impl ResetValue for RAR

Register rar `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RAR

`read()` method returns rar::R reader structure

source

### impl Writable for RAR

`write(|w| ..)` method takes rar::W writer structure