# RFCR in k210_pac::i2s0::channel - Rust
Receive FIFO Configuration Register
Keywords: rust, rustlang, rust-lang, RFCR

# Type Definition k210_pac::i2s0::channel::RFCR

source · [−]

    pub type RFCR = Reg<u32, _RFCR>;

Expand description

Receive FIFO Configuration Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rfcr module

## Trait Implementations

source

### impl ResetValue for RFCR

Register rfcr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RFCR

`read()` method returns rfcr::R reader structure

source

### impl Writable for RFCR

`write(|w| ..)` method takes rfcr::W writer structure