# DMA_RDLR in k210_pac::i2c0 - Rust
DMA Receive Data Level Register
Keywords: rust, rustlang, rust-lang, DMA_RDLR

# Type Definition k210_pac::i2c0::DMA_RDLR

source · [−]

    pub type DMA_RDLR = Reg<u32, _DMA_RDLR>;

Expand description

DMA Receive Data Level Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see dma_rdlr module

## Trait Implementations

source

### impl ResetValue for DMA_RDLR

Register dma_rdlr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DMA_RDLR

`read()` method returns dma_rdlr::R reader structure

source

### impl Writable for DMA_RDLR

`write(|w| ..)` method takes dma_rdlr::W writer structure