# DATA_IN_FLAG in k210_pac::aes - Rust
Data can input flag
Keywords: rust, rustlang, rust-lang, DATA_IN_FLAG

# Type Definition k210_pac::aes::DATA_IN_FLAG

source · [−]

    pub type DATA_IN_FLAG = Reg<u32, _DATA_IN_FLAG>;

Expand description

Data can input flag

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see data_in_flag module

## Trait Implementations

source

### impl ResetValue for DATA_IN_FLAG

Register data_in_flag `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DATA_IN_FLAG

`read()` method returns data_in_flag::R reader structure

source

### impl Writable for DATA_IN_FLAG

`write(|w| ..)` method takes data_in_flag::W writer structure