# MCR in k210_pac::uart1 - Rust
Modem Control Register
Keywords: rust, rustlang, rust-lang, MCR

# Type Definition k210_pac::uart1::MCR

source · [−]

    pub type MCR = Reg<u32, _MCR>;

Expand description

Modem Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see mcr module

## Trait Implementations

source

### impl ResetValue for MCR

Register mcr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for MCR

`read()` method returns mcr::R reader structure

source

### impl Writable for MCR

`write(|w| ..)` method takes mcr::W writer structure