# LEFT_RXTX in k210_pac::i2s0::channel - Rust
Left Receive or Left Transmit Register
Keywords: rust, rustlang, rust-lang, LEFT_RXTX

# Type Definition k210_pac::i2s0::channel::LEFT_RXTX

source · [−]

    pub type LEFT_RXTX = Reg<u32, _LEFT_RXTX>;

Expand description

Left Receive or Left Transmit Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see left_rxtx module

## Trait Implementations

source

### impl ResetValue for LEFT_RXTX

Register left_rxtx `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for LEFT_RXTX

`read()` method returns left_rxtx::R reader structure

source

### impl Writable for LEFT_RXTX

`write(|w| ..)` method takes left_rxtx::W writer structure