# RX_TL in k210_pac::i2c0 - Rust
Receive FIFO Threshold Register
Keywords: rust, rustlang, rust-lang, RX_TL

# Type Definition k210_pac::i2c0::RX_TL

source · [−]

    pub type RX_TL = Reg<u32, _RX_TL>;

Expand description

Receive FIFO Threshold Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rx_tl module

## Trait Implementations

source

### impl ResetValue for RX_TL

Register rx_tl `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RX_TL

`read()` method returns rx_tl::R reader structure

source

### impl Writable for RX_TL

`write(|w| ..)` method takes rx_tl::W writer structure