# I2S_COMP_VERSION_1 in k210_pac::i2s0 - Rust
Component Version Register
Keywords: rust, rustlang, rust-lang, I2S_COMP_VERSION_1

# Type Definition k210_pac::i2s0::I2S_COMP_VERSION_1

source · [−]

    pub type I2S_COMP_VERSION_1 = Reg<u32, _I2S_COMP_VERSION_1>;

Expand description

Component Version Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see i2s_comp_version_1 module

## Trait Implementations

source

### impl ResetValue for I2S_COMP_VERSION_1

Register i2s_comp_version_1 `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for I2S_COMP_VERSION_1

`read()` method returns i2s_comp_version_1::R reader structure

source

### impl Writable for I2S_COMP_VERSION_1

`write(|w| ..)` method takes i2s_comp_version_1::W writer structure