# RXFFR in k210_pac::i2s0 - Rust
Receiver Block FIFO Reset Register
Keywords: rust, rustlang, rust-lang, RXFFR

# Type Definition k210_pac::i2s0::RXFFR

source · [−]

    pub type RXFFR = Reg<u32, _RXFFR>;

Expand description

Receiver Block FIFO Reset Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxffr module

## Trait Implementations

source

### impl ResetValue for RXFFR

Register rxffr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXFFR

`read()` method returns rxffr::R reader structure

source

### impl Writable for RXFFR

`write(|w| ..)` method takes rxffr::W writer structure