# R in k210_pac::dvp::sccb_ctl - Rust
Reader of register sccb_ctl
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::dvp::sccb_ctl::R

source · [−]

    pub type R = R<u32, SCCB_CTL>;

Expand description

Reader of register sccb_ctl

## Implementations

source

### impl R

source

#### pub fn device_address(&self) -> DEVICE_ADDRESS_R

Bits 0:7 - DEVICE_ADDRESS

source

#### pub fn reg_address(&self) -> REG_ADDRESS_R

Bits 8:15 - REG_ADDRESS

source

#### pub fn wdata_byte0(&self) -> WDATA_BYTE0_R

Bits 16:23 - WDATA_BYTE0

source

#### pub fn wdata_byte1(&self) -> WDATA_BYTE1_R

Bits 24:31 - WDATA_BYTE1