# POWER_SEL in k210_pac::sysctl - Rust
IO Power Mode Select controller
Keywords: rust, rustlang, rust-lang, POWER_SEL

# Type Definition k210_pac::sysctl::POWER_SEL

source · [−]

    pub type POWER_SEL = Reg<u32, _POWER_SEL>;

Expand description

IO Power Mode Select controller

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see power_sel module

## Trait Implementations

source

### impl ResetValue for POWER_SEL

Register power_sel `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for POWER_SEL

`read()` method returns power_sel::R reader structure

source

### impl Writable for POWER_SEL

`write(|w| ..)` method takes power_sel::W writer structure