# RISR in k210_pac::spi3 - Rust
Raw Interrupt Status Register
Keywords: rust, rustlang, rust-lang, RISR

# Type Definition k210_pac::spi3::RISR

source · [−]

    pub type RISR = Reg<u32, _RISR>;

Expand description

Raw Interrupt Status Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see risr module

## Trait Implementations

source

### impl ResetValue for RISR

Register risr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RISR

`read()` method returns risr::R reader structure

source

### impl Writable for RISR

`write(|w| ..)` method takes risr::W writer structure