# DMACR in k210_pac::spi3 - Rust
DMA Control Register
Keywords: rust, rustlang, rust-lang, DMACR

# Type Definition k210_pac::spi3::DMACR

source · [−]

    pub type DMACR = Reg<u32, _DMACR>;

Expand description

DMA Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see dmacr module

## Trait Implementations

source

### impl ResetValue for DMACR

Register dmacr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DMACR

`read()` method returns dmacr::R reader structure

source

### impl Writable for DMACR

`write(|w| ..)` method takes dmacr::W writer structure