# VOBUF_DMA_RDATA in k210_pac::apu - Rust
Read register for DMA to voice-out buffers
Keywords: rust, rustlang, rust-lang, VOBUF_DMA_RDATA

# Type Definition k210_pac::apu::VOBUF_DMA_RDATA

source · [−]

    pub type VOBUF_DMA_RDATA = Reg<u32, _VOBUF_DMA_RDATA>;

Expand description

Read register for DMA to voice-out buffers

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see vobuf_dma_rdata module

## Trait Implementations

source

### impl ResetValue for VOBUF_DMA_RDATA

Register vobuf_dma_rdata `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for VOBUF_DMA_RDATA

`read()` method returns vobuf_dma_rdata::R reader structure

source

### impl Writable for VOBUF_DMA_RDATA

`write(|w| ..)` method takes vobuf_dma_rdata::W writer structure