# GCM_OUT_TAG in k210_pac::aes - Rust
Computed GCM output tag
Keywords: rust, rustlang, rust-lang, GCM_OUT_TAG

# Type Definition k210_pac::aes::GCM_OUT_TAG

source · [−]

    pub type GCM_OUT_TAG = Reg<u32, _GCM_OUT_TAG>;

Expand description

Computed GCM output tag

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see gcm_out_tag module

## Trait Implementations

source

### impl ResetValue for GCM_OUT_TAG

Register gcm_out_tag[%s] `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for GCM_OUT_TAG

`read()` method returns gcm_out_tag::R reader structure

source

### impl Writable for GCM_OUT_TAG

`write(|w| ..)` method takes gcm_out_tag::W writer structure