# INTR_STAT in k210_pac::timer0 - Rust
Interrupt Status Register
Keywords: rust, rustlang, rust-lang, INTR_STAT

# Type Definition k210_pac::timer0::INTR_STAT

source · [−]

    pub type INTR_STAT = Reg<u32, _INTR_STAT>;

Expand description

Interrupt Status Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see intr_stat module

## Trait Implementations

source

### impl ResetValue for INTR_STAT

Register intr_stat `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for INTR_STAT

`read()` method returns intr_stat::R reader structure

source

### impl Writable for INTR_STAT

`write(|w| ..)` method takes intr_stat::W writer structure