# TXDMA in k210_pac::i2s0 - Rust
Transmitter Block DMA Register
Keywords: rust, rustlang, rust-lang, TXDMA

# Type Definition k210_pac::i2s0::TXDMA

source · [−]

    pub type TXDMA = Reg<u32, _TXDMA>;

Expand description

Transmitter Block DMA Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see txdma module

## Trait Implementations

source

### impl ResetValue for TXDMA

Register txdma `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for TXDMA

`read()` method returns txdma::R reader structure

source

### impl Writable for TXDMA

`write(|w| ..)` method takes txdma::W writer structure