# SRT in k210_pac::uart1 - Rust
Shadow RCVR Trigger Register
Keywords: rust, rustlang, rust-lang, SRT

# Type Definition k210_pac::uart1::SRT

source · [−]

    pub type SRT = Reg<u32, _SRT>;

Expand description

Shadow RCVR Trigger Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see srt module

## Trait Implementations

source

### impl ResetValue for SRT

Register srt `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SRT

`read()` method returns srt::R reader structure

source

### impl Writable for SRT

`write(|w| ..)` method takes srt::W writer structure