# INTERRUPT_STATUS in k210_pac::kpu - Rust
Interrupt status
Keywords: rust, rustlang, rust-lang, INTERRUPT_STATUS

# Type Definition k210_pac::kpu::INTERRUPT_STATUS

source · [−]

    pub type INTERRUPT_STATUS = Reg<u64, _INTERRUPT_STATUS>;

Expand description

Interrupt status

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see interrupt_status module

## Trait Implementations

source

### impl ResetValue for INTERRUPT_STATUS

Register interrupt_status `reset()`’s with value 0

#### type Type = u64

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for INTERRUPT_STATUS

`read()` method returns interrupt_status::R reader structure

source

### impl Writable for INTERRUPT_STATUS

`write(|w| ..)` method takes interrupt_status::W writer structure