# CTRLR0 in k210_pac::spi3 - Rust
Control Register 0
Keywords: rust, rustlang, rust-lang, CTRLR0

# Type Definition k210_pac::spi3::CTRLR0

source · [−]

    pub type CTRLR0 = Reg<u32, _CTRLR0>;

Expand description

Control Register 0

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ctrlr0 module

## Trait Implementations

source

### impl ResetValue for CTRLR0

Register ctrlr0 `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CTRLR0

`read()` method returns ctrlr0::R reader structure

source

### impl Writable for CTRLR0

`write(|w| ..)` method takes ctrlr0::W writer structure