# INTERRUPT_BOTHEDGE in k210_pac::gpio - Rust
Interrupt both edge type
Keywords: rust, rustlang, rust-lang, INTERRUPT_BOTHEDGE

# Type Definition k210_pac::gpio::INTERRUPT_BOTHEDGE

source · [−]

    pub type INTERRUPT_BOTHEDGE = Reg<u32, _INTERRUPT_BOTHEDGE>;

Expand description

Interrupt both edge type

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see interrupt_bothedge module

## Trait Implementations

source

### impl ResetValue for INTERRUPT_BOTHEDGE

Register interrupt_bothedge `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for INTERRUPT_BOTHEDGE

`read()` method returns interrupt_bothedge::R reader structure

source

### impl Writable for INTERRUPT_BOTHEDGE

`write(|w| ..)` method takes interrupt_bothedge::W writer structure