# RXDMA in k210_pac::i2s0 - Rust
Receiver Block DMA Register
Keywords: rust, rustlang, rust-lang, RXDMA

# Type Definition k210_pac::i2s0::RXDMA

source · [−]

    pub type RXDMA = Reg<u32, _RXDMA>;

Expand description

Receiver Block DMA Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxdma module

## Trait Implementations

source

### impl ResetValue for RXDMA

Register rxdma `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXDMA

`read()` method returns rxdma::R reader structure

source

### impl Writable for RXDMA

`write(|w| ..)` method takes rxdma::W writer structure