# I2S_COMP_TYPE in k210_pac::i2s0 - Rust
Component Type Register
Keywords: rust, rustlang, rust-lang, I2S_COMP_TYPE

# Type Definition k210_pac::i2s0::I2S_COMP_TYPE

source · [−]

    pub type I2S_COMP_TYPE = Reg<u32, _I2S_COMP_TYPE>;

Expand description

Component Type Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see i2s_comp_type module

## Trait Implementations

source

### impl ResetValue for I2S_COMP_TYPE

Register i2s_comp_type `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for I2S_COMP_TYPE

`read()` method returns i2s_comp_type::R reader structure

source

### impl Writable for I2S_COMP_TYPE

`write(|w| ..)` method takes i2s_comp_type::W writer structure