# SS_SCL_LCNT in k210_pac::i2c0 - Rust
Standard Speed Clock SCL Low Count Register
Keywords: rust, rustlang, rust-lang, SS_SCL_LCNT

# Type Definition k210_pac::i2c0::SS_SCL_LCNT

source · [−]

    pub type SS_SCL_LCNT = Reg<u32, _SS_SCL_LCNT>;

Expand description

Standard Speed Clock SCL Low Count Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ss_scl_lcnt module

## Trait Implementations

source

### impl ResetValue for SS_SCL_LCNT

Register ss_scl_lcnt `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SS_SCL_LCNT

`read()` method returns ss_scl_lcnt::R reader structure

source

### impl Writable for SS_SCL_LCNT

`write(|w| ..)` method takes ss_scl_lcnt::W writer structure