# UCV in k210_pac::uart1 - Rust
UART Component Version
Keywords: rust, rustlang, rust-lang, UCV

# Type Definition k210_pac::uart1::UCV

source · [−]

    pub type UCV = Reg<u32, _UCV>;

Expand description

UART Component Version

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ucv module

## Trait Implementations

source

### impl ResetValue for UCV

Register ucv `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for UCV

`read()` method returns ucv::R reader structure

source

### impl Writable for UCV

`write(|w| ..)` method takes ucv::W writer structure