# CCR in k210_pac::i2s0 - Rust
Clock Configuration Register
Keywords: rust, rustlang, rust-lang, CCR

# Type Definition k210_pac::i2s0::CCR

source · [−]

    pub type CCR = Reg<u32, _CCR>;

Expand description

Clock Configuration Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see ccr module

## Trait Implementations

source

### impl ResetValue for CCR

Register ccr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CCR

`read()` method returns ccr::R reader structure

source

### impl Writable for CCR

`write(|w| ..)` method takes ccr::W writer structure