# TX_TL in k210_pac::i2c0 - Rust
Transmit FIFO Threshold Register
Keywords: rust, rustlang, rust-lang, TX_TL

# Type Definition k210_pac::i2c0::TX_TL

source · [−]

    pub type TX_TL = Reg<u32, _TX_TL>;

Expand description

Transmit FIFO Threshold Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see tx_tl module

## Trait Implementations

source

### impl ResetValue for TX_TL

Register tx_tl `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for TX_TL

`read()` method returns tx_tl::R reader structure

source

### impl Writable for TX_TL

`write(|w| ..)` method takes tx_tl::W writer structure