# RXFTLR in k210_pac::spi0 - Rust
Receive FIFO Threshold Level
Keywords: rust, rustlang, rust-lang, RXFTLR

# Type Definition k210_pac::spi0::RXFTLR

source · [−]

    pub type RXFTLR = Reg<u32, _RXFTLR>;

Expand description

Receive FIFO Threshold Level

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxftlr module

## Trait Implementations

source

### impl ResetValue for RXFTLR

Register rxftlr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXFTLR

`read()` method returns rxftlr::R reader structure

source

### impl Writable for RXFTLR

`write(|w| ..)` method takes rxftlr::W writer structure