# R in k210_pac::i2c0::enable_status - Rust
Reader of register enable_status
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::i2c0::enable_status::R

source · [−]

    pub type R = R<u32, ENABLE_STATUS>;

Expand description

Reader of register enable_status

## Implementations

source

### impl R

source

#### pub fn ic_enable(&self) -> IC_ENABLE_R

Bit 0 - IC_ENABLE

source

#### pub fn slv_dis_busy(&self) -> SLV_DIS_BUSY_R

Bit 1 - SLV_DIS_BUSY

source

#### pub fn slv_rx_data_lost(&self) -> SLV_RX_DATA_LOST_R

Bit 2 - SLV_RX_DATA_LOST