# DMA_SEL0_R in k210_pac::sysctl::dma_sel0 - Rust
Reader of field `dma_sel0`
Keywords: rust, rustlang, rust-lang, DMA_SEL0_R

# Type Definition k210_pac::sysctl::dma_sel0::DMA_SEL0_R

source · [−]

    pub type DMA_SEL0_R = R<u8, DMA_SEL0_A>;

Expand description

Reader of field `dma_sel0`

## Implementations

source

### impl DMA_SEL0_R

source

#### pub fn variant(&self) -> Variant<u8, DMA_SEL0_A>

Get enumerated values variant

source

#### pub fn is_ssi0_rx_req(&self) -> bool

Checks if the value of the field is `SSI0_RX_REQ`

source

#### pub fn is_ssi0_tx_req(&self) -> bool

Checks if the value of the field is `SSI0_TX_REQ`

source

#### pub fn is_ssi1_rx_req(&self) -> bool

Checks if the value of the field is `SSI1_RX_REQ`

source

#### pub fn is_ssi1_tx_req(&self) -> bool

Checks if the value of the field is `SSI1_TX_REQ`

source

#### pub fn is_ssi2_rx_req(&self) -> bool

Checks if the value of the field is `SSI2_RX_REQ`

source

#### pub fn is_ssi2_tx_req(&self) -> bool

Checks if the value of the field is `SSI2_TX_REQ`

source

#### pub fn is_ssi3_rx_req(&self) -> bool

Checks if the value of the field is `SSI3_RX_REQ`

source

#### pub fn is_ssi3_tx_req(&self) -> bool

Checks if the value of the field is `SSI3_TX_REQ`

source

#### pub fn is_i2c0_rx_req(&self) -> bool

Checks if the value of the field is `I2C0_RX_REQ`

source

#### pub fn is_i2c0_tx_req(&self) -> bool

Checks if the value of the field is `I2C0_TX_REQ`

source

#### pub fn is_i2c1_rx_req(&self) -> bool

Checks if the value of the field is `I2C1_RX_REQ`

source

#### pub fn is_i2c1_tx_req(&self) -> bool

Checks if the value of the field is `I2C1_TX_REQ`

source

#### pub fn is_i2c2_rx_req(&self) -> bool

Checks if the value of the field is `I2C2_RX_REQ`

source

#### pub fn is_i2c2_tx_req(&self) -> bool

Checks if the value of the field is `I2C2_TX_REQ`

source

#### pub fn is_uart1_rx_req(&self) -> bool

Checks if the value of the field is `UART1_RX_REQ`

source

#### pub fn is_uart1_tx_req(&self) -> bool

Checks if the value of the field is `UART1_TX_REQ`

source

#### pub fn is_uart2_rx_req(&self) -> bool

Checks if the value of the field is `UART2_RX_REQ`

source

#### pub fn is_uart2_tx_req(&self) -> bool

Checks if the value of the field is `UART2_TX_REQ`

source

#### pub fn is_uart3_rx_req(&self) -> bool

Checks if the value of the field is `UART3_RX_REQ`

source

#### pub fn is_uart3_tx_req(&self) -> bool

Checks if the value of the field is `UART3_TX_REQ`

source

#### pub fn is_aes_req(&self) -> bool

Checks if the value of the field is `AES_REQ`

source

#### pub fn is_sha_rx_req(&self) -> bool

Checks if the value of the field is `SHA_RX_REQ`

source

#### pub fn is_ai_rx_req(&self) -> bool

Checks if the value of the field is `AI_RX_REQ`

source

#### pub fn is_fft_rx_req(&self) -> bool

Checks if the value of the field is `FFT_RX_REQ`

source

#### pub fn is_fft_tx_req(&self) -> bool

Checks if the value of the field is `FFT_TX_REQ`

source

#### pub fn is_i2s0_tx_req(&self) -> bool

Checks if the value of the field is `I2S0_TX_REQ`

source

#### pub fn is_i2s0_rx_req(&self) -> bool

Checks if the value of the field is `I2S0_RX_REQ`

source

#### pub fn is_i2s1_tx_req(&self) -> bool

Checks if the value of the field is `I2S1_TX_REQ`

source

#### pub fn is_i2s1_rx_req(&self) -> bool

Checks if the value of the field is `I2S1_RX_REQ`

source

#### pub fn is_i2s2_tx_req(&self) -> bool

Checks if the value of the field is `I2S2_TX_REQ`

source

#### pub fn is_i2s2_rx_req(&self) -> bool

Checks if the value of the field is `I2S2_RX_REQ`

source

#### pub fn is_i2s0_bf_dir_req(&self) -> bool

Checks if the value of the field is `I2S0_BF_DIR_REQ`

source

#### pub fn is_i2s0_bf_voice_req(&self) -> bool

Checks if the value of the field is `I2S0_BF_VOICE_REQ`