# SDA_SETUP in k210_pac::i2c0 - Rust
SDA Setup Register
Keywords: rust, rustlang, rust-lang, SDA_SETUP

# Type Definition k210_pac::i2c0::SDA_SETUP

source · [−]

    pub type SDA_SETUP = Reg<u32, _SDA_SETUP>;

Expand description

SDA Setup Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see sda_setup module

## Trait Implementations

source

### impl ResetValue for SDA_SETUP

Register sda_setup `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for SDA_SETUP

`read()` method returns sda_setup::R reader structure

source

### impl Writable for SDA_SETUP

`write(|w| ..)` method takes sda_setup::W writer structure