# DMA_CR in k210_pac::i2c0 - Rust
I2C DMA Control Register
Keywords: rust, rustlang, rust-lang, DMA_CR

# Type Definition k210_pac::i2c0::DMA_CR

source · [−]

    pub type DMA_CR = Reg<u32, _DMA_CR>;

Expand description

I2C DMA Control Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see dma_cr module

## Trait Implementations

source

### impl ResetValue for DMA_CR

Register dma_cr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for DMA_CR

`read()` method returns dma_cr::R reader structure

source

### impl Writable for DMA_CR

`write(|w| ..)` method takes dma_cr::W writer structure