# k210_pac::sysctl::power_sel - Rust
IO Power Mode Select controller
Keywords: rust, rustlang, rust-lang, power_sel

# Module k210_pac::sysctl::power_sel

source · [−]
Expand description

IO Power Mode Select controller

## Structs

POWER_MODE_SEL0_W

Write proxy for field `power_mode_sel0`

POWER_MODE_SEL1_W

Write proxy for field `power_mode_sel1`

POWER_MODE_SEL2_W

Write proxy for field `power_mode_sel2`

POWER_MODE_SEL3_W

Write proxy for field `power_mode_sel3`

POWER_MODE_SEL4_W

Write proxy for field `power_mode_sel4`

POWER_MODE_SEL5_W

Write proxy for field `power_mode_sel5`

POWER_MODE_SEL6_W

Write proxy for field `power_mode_sel6`

POWER_MODE_SEL7_W

Write proxy for field `power_mode_sel7`

## Type Definitions

POWER_MODE_SEL0_R

Reader of field `power_mode_sel0`

POWER_MODE_SEL1_R

Reader of field `power_mode_sel1`

POWER_MODE_SEL2_R

Reader of field `power_mode_sel2`

POWER_MODE_SEL3_R

Reader of field `power_mode_sel3`

POWER_MODE_SEL4_R

Reader of field `power_mode_sel4`

POWER_MODE_SEL5_R

Reader of field `power_mode_sel5`

POWER_MODE_SEL6_R

Reader of field `power_mode_sel6`

POWER_MODE_SEL7_R

Reader of field `power_mode_sel7`

R

Reader of register power_sel

W

Writer for register power_sel