# CLK_TH3 in k210_pac::sysctl - Rust
Clock threshold controller 3
Keywords: rust, rustlang, rust-lang, CLK_TH3

# Type Definition k210_pac::sysctl::CLK_TH3

source · [−]

    pub type CLK_TH3 = Reg<u32, _CLK_TH3>;

Expand description

Clock threshold controller 3

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see clk_th3 module

## Trait Implementations

source

### impl ResetValue for CLK_TH3

Register clk_th3 `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CLK_TH3

`read()` method returns clk_th3::R reader structure

source

### impl Writable for CLK_TH3

`write(|w| ..)` method takes clk_th3::W writer structure