# XIP_CNT_TIME_OUT in k210_pac::spi3 - Rust
XIP time out register for continuous transfers
Keywords: rust, rustlang, rust-lang, XIP_CNT_TIME_OUT

# Type Definition k210_pac::spi3::XIP_CNT_TIME_OUT

source · [−]

    pub type XIP_CNT_TIME_OUT = Reg<u32, _XIP_CNT_TIME_OUT>;

Expand description

XIP time out register for continuous transfers

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see xip_cnt_time_out module

## Trait Implementations

source

### impl ResetValue for XIP_CNT_TIME_OUT

Register xip_cnt_time_out `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for XIP_CNT_TIME_OUT

`read()` method returns xip_cnt_time_out::R reader structure

source

### impl Writable for XIP_CNT_TIME_OUT

`write(|w| ..)` method takes xip_cnt_time_out::W writer structure