# RTXDMA in k210_pac::i2s0 - Rust
Reset Transmitter Block DMA Register
Keywords: rust, rustlang, rust-lang, RTXDMA

# Type Definition k210_pac::i2s0::RTXDMA

source · [−]

    pub type RTXDMA = Reg<u32, _RTXDMA>;

Expand description

Reset Transmitter Block DMA Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rtxdma module

## Trait Implementations

source

### impl ResetValue for RTXDMA

Register rtxdma `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RTXDMA

`read()` method returns rtxdma::R reader structure

source

### impl Writable for RTXDMA

`write(|w| ..)` method takes rtxdma::W writer structure