# TAR in k210_pac::i2c0 - Rust
Target Address Register
Keywords: rust, rustlang, rust-lang, TAR

# Type Definition k210_pac::i2c0::TAR

source · [−]

    pub type TAR = Reg<u32, _TAR>;

Expand description

Target Address Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see tar module

## Trait Implementations

source

### impl ResetValue for TAR

Register tar `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for TAR

`read()` method returns tar::R reader structure

source

### impl Writable for TAR

`write(|w| ..)` method takes tar::W writer structure