# INTERRUPT_CTRL in k210_pac::rtc - Rust
RTC interrupt settings
Keywords: rust, rustlang, rust-lang, INTERRUPT_CTRL

# Type Definition k210_pac::rtc::INTERRUPT_CTRL

source · [−]

    pub type INTERRUPT_CTRL = Reg<u32, _INTERRUPT_CTRL>;

Expand description

RTC interrupt settings

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see interrupt_ctrl module

## Trait Implementations

source

### impl ResetValue for INTERRUPT_CTRL

Register interrupt_ctrl `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for INTERRUPT_CTRL

`read()` method returns interrupt_ctrl::R reader structure

source

### impl Writable for INTERRUPT_CTRL

`write(|w| ..)` method takes interrupt_ctrl::W writer structure