# R in k210_pac::sysctl::peri - Rust
Reader of register peri
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::sysctl::peri::R

source · [−]

    pub type R = R<u32, PERI>;

Expand description

Reader of register peri

## Implementations

source

### impl R

source

#### pub fn timer0_pause(&self) -> TIMER0_PAUSE_R

Bit 0

source

#### pub fn timer1_pause(&self) -> TIMER1_PAUSE_R

Bit 1

source

#### pub fn timer2_pause(&self) -> TIMER2_PAUSE_R

Bit 2

source

#### pub fn timer3_pause(&self) -> TIMER3_PAUSE_R

Bit 3

source

#### pub fn timer4_pause(&self) -> TIMER4_PAUSE_R

Bit 4

source

#### pub fn timer5_pause(&self) -> TIMER5_PAUSE_R

Bit 5

source

#### pub fn timer6_pause(&self) -> TIMER6_PAUSE_R

Bit 6

source

#### pub fn timer7_pause(&self) -> TIMER7_PAUSE_R

Bit 7

source

#### pub fn timer8_pause(&self) -> TIMER8_PAUSE_R

Bit 8

source

#### pub fn timer9_pause(&self) -> TIMER9_PAUSE_R

Bit 9

source

#### pub fn timer10_pause(&self) -> TIMER10_PAUSE_R

Bit 10

source

#### pub fn timer11_pause(&self) -> TIMER11_PAUSE_R

Bit 11

source

#### pub fn spi0_xip_en(&self) -> SPI0_XIP_EN_R

Bit 12

source

#### pub fn spi1_xip_en(&self) -> SPI1_XIP_EN_R

Bit 13

source

#### pub fn spi2_xip_en(&self) -> SPI2_XIP_EN_R

Bit 14

source

#### pub fn spi3_xip_en(&self) -> SPI3_XIP_EN_R

Bit 15

source

#### pub fn spi0_clk_bypass(&self) -> SPI0_CLK_BYPASS_R

Bit 16

source

#### pub fn spi1_clk_bypass(&self) -> SPI1_CLK_BYPASS_R

Bit 17

source

#### pub fn spi2_clk_bypass(&self) -> SPI2_CLK_BYPASS_R

Bit 18

source

#### pub fn i2s0_clk_bypass(&self) -> I2S0_CLK_BYPASS_R

Bit 19

source

#### pub fn i2s1_clk_bypass(&self) -> I2S1_CLK_BYPASS_R

Bit 20

source

#### pub fn i2s2_clk_bypass(&self) -> I2S2_CLK_BYPASS_R

Bit 21

source

#### pub fn jtag_clk_bypass(&self) -> JTAG_CLK_BYPASS_R

Bit 22

source

#### pub fn dvp_clk_bypass(&self) -> DVP_CLK_BYPASS_R

Bit 23

source

#### pub fn debug_clk_bypass(&self) -> DEBUG_CLK_BYPASS_R

Bit 24