# CER in k210_pac::i2s0 - Rust
Clock Generation enable
Keywords: rust, rustlang, rust-lang, CER

# Type Definition k210_pac::i2s0::CER

source · [−]

    pub type CER = Reg<u32, _CER>;

Expand description

Clock Generation enable

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see cer module

## Trait Implementations

source

### impl ResetValue for CER

Register cer `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for CER

`read()` method returns cer::R reader structure

source

### impl Writable for CER

`write(|w| ..)` method takes cer::W writer structure