# RXOICR in k210_pac::spi3 - Rust
Receive FIFO Overflow Interrupt Clear Register
Keywords: rust, rustlang, rust-lang, RXOICR

# Type Definition k210_pac::spi3::RXOICR

source · [−]

    pub type RXOICR = Reg<u32, _RXOICR>;

Expand description

Receive FIFO Overflow Interrupt Clear Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see rxoicr module

## Trait Implementations

source

### impl ResetValue for RXOICR

Register rxoicr `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for RXOICR

`read()` method returns rxoicr::R reader structure

source

### impl Writable for RXOICR

`write(|w| ..)` method takes rxoicr::W writer structure