# R in k210_pac::i2c0::status - Rust
Reader of register status
Keywords: rust, rustlang, rust-lang, R

# Type Definition k210_pac::i2c0::status::R

source · [−]

    pub type R = R<u32, STATUS>;

Expand description

Reader of register status

## Implementations

source

### impl R

source

#### pub fn activity(&self) -> ACTIVITY_R

Bit 0 - ACTIVITY

source

#### pub fn tfnf(&self) -> TFNF_R

Bit 1 - TFNF

source

#### pub fn tfe(&self) -> TFE_R

Bit 2 - TFE

source

#### pub fn rfne(&self) -> RFNE_R

Bit 3 - RFNE

source

#### pub fn rff(&self) -> RFF_R

Bit 4 - RFF

source

#### pub fn mst_activity(&self) -> MST_ACTIVITY_R

Bit 5 - MST_ACTIVITY

source

#### pub fn slv_activity(&self) -> SLV_ACTIVITY_R

Bit 6 - SLV_ACTIVITY