# GENERAL_CALL in k210_pac::i2c0 - Rust
ACK General Call Register
Keywords: rust, rustlang, rust-lang, GENERAL_CALL

# Type Definition k210_pac::i2c0::GENERAL_CALL

source · [−]

    pub type GENERAL_CALL = Reg<u32, _GENERAL_CALL>;

Expand description

ACK General Call Register

This register you can `read`, `reset`, `write`, `write_with_zero`, `modify`. See API.

For information about available fields see general_call module

## Trait Implementations

source

### impl ResetValue for GENERAL_CALL

Register general_call `reset()`’s with value 0

#### type Type = u32

Raw register type (`u8`, `u16`, `u32`, …).

source

#### fn reset_value() -> Self::Type

Reset value of the register.

source

### impl Readable for GENERAL_CALL

`read()` method returns general_call::R reader structure

source

### impl Writable for GENERAL_CALL

`write(|w| ..)` method takes general_call::W writer structure